Program to add two 16 bit numbers

DATA SEGMENT

A1 DW 0FFFFH

A2 DW 1232H

A3 DW 0000H

A4 DB 00H

DATA ENDS

CODE SEGMENT

ASSUME CS:CODE,DS:DATA

START: MOV AX,DATA

 MOV DS,AX

 MOV DL,00H

 MOV AX,A1

 MOV BX,A2

 ADD AX,BX

 JNC NEXT

 INC DL

 NEXT: MOV A3,AX

 MOV A4,DL

 INT 3

CODE ENDS

 END START

Program to subtract two 16 bit numbers

DATA SEGMENT

A1 DW 0FFFFH

A2 DW 1232H

A3 DW 0000H

DATA ENDS

CODE SEGMENT

ASSUME CS:CODE,DS:DATA

START: MOV AX,DATA

 MOV DS,AX

 MOV AX,A1

 MOV BX,A2

 SUB AX,BX

 MOV A3,AX

 INT 3

CODE ENDS

 END START

Program to multiply two 16 bit numbers

DATA SEGMENT

A1 DW 2345H

A2 DW 1232H

A3 DW 0000H

A4 DW 0000H

DATA ENDS

CODE SEGMENT

ASSUME CS:CODE,DS:DATA

START: MOV AX,DATA

 MOV DS,AX

 MOV AX,A1

 MOV BX,A2

 MUL BX

 MOV A3,AX

 MOV A4,DX

 INT 3

CODE ENDS

 END START

Program to divide a 32 bit number by 16 bit number

DATA SEGMENT

A1 DW 2345H

A2 DW 1232H

A3 DW 0FF34H

A4 DW 0000H

A5 DW 0000H

DATA ENDS

CODE SEGMENT

ASSUME CS:CODE,DS:DATA

START: MOV AX,DATA

 MOV DS,AX

 MOV AX,A1

 MOV DX,A2

 MOV BX,A3

 DIV BX

 MOV A4,AX

 MOV A5,DX

 INT 3

CODE ENDS

 END START